**Article Title Georgia Size 22 Points not include abbreviation as possible**

Capitalize Each word except for prepositions

example (the, in, it, on, in, of, using, as, a, an, with, etc.)

**First name M. I. Surnamea,\* , First name A. I. Surname b, First name M. I. Surnamea**

aElectrical Department/ Engineering College/Tikrit University /Tikrit, Iraq

Email: [xxxxx@xxx.com](mailto:xxxxx@xxx.com); ORCID: <https://orcid.org/xxxx-xxxx-xxxx-xxxx>

bDepartment of Chemical Engineering/College of Engineering /Tikrit University/ Tikrit/ Iraq

Email: [xxxx@xxx.com](mailto:xxxx@xxx.com), ORCID: <https://orcid.org/xxxx-xxxx-xxxx-xxxx>

**هاشم علي اسماعيل قسم الهندسة المدنية/ كلية هندسة / جامعة تكريت وسعد حامد محمد قسم الهندسة الكيميائية/كلية الهندسة / جامعة الموصل**

**ABSTRACT**

The maximum length of the abstract is 350 words. No literature references should be contained in the abstract. The abstract should briefly state the objective and approach and give a succinct summary of results and major conclusions should be drawn in one paragraph and a single column. Emphasis should be on what was found, not what was done. Paste your abstract here (paste form option choose merge format). Keywords must be arranged alphabetically and not less than 5 keywords should be written.

***Keywords*:** Cobalt, Iron oxide, Magnetic flocculation, Nickel, Oil refineries wastewater.

Abstract: one paragraph only

Keywords: min. (5) words and max. (7) words, and arrange it alphabetically

تكون الخلاصة فقرة واحدة والكلمات الدالة من 5 الى 7 كلمات مرتبة ابجديا

**Highlights**

-Structural performance of HSC Reinforced with HGFRP bars with steel wires.

-Structural performance was considered in experimental & NLFEA manners

-NLFEA was done using Ansys 2019-R1.

**-**

***Highlights***

Highlights are 3-5 bullet points that help increase the discoverability of your article via search engines. These bullet points should capture the novel results of your research as well as new methods that were used during the study (if any). Think of them as the "elevator pitch" of your article. Please include terms that you know your readers will be looking for online. Don't try to capture all ideas, concepts or conclusions as highlights are meant to be short: 85 characters or fewer, including spaces.

النقاط البارزة في البحث

النقاط البارزة هي 3-5 نقاط تساعد على زيادة قابلية اكتشاف مقالك عبر محركات البحث. يجب أن تلخص النقاط البارزة النتائج والاستنتاجات الجديدة لبحثك وكذلك الطرق الجديدة والاصالة التي تم استخدامها خلال الدراسة (إن وجدت). فكر فيهم على أنهم "محرك الصعود" لمقالك. يرجى تضمين المصطلحات التي يعرفها الباحثين في الانترنيت. لا تحاول التقاط جميع الأفكار أو المفاهيم أو الاستنتاجات لأن النقاط البارزة تهدف إلى أن تكون قصيرة: 85 حرفًا أو أقل ، بما في ذلك المساحات.

**CREDIT AUTHORSHIP CONTRIBUTION STATEMENT**

***Qian Ren***: Writing – original draft, Visualization, Validation, Methodology, Investigation, Formal analysis, Data curation, Conceptualization. ***Xiaoyu Zhang***: Methodology, Investigation. ***Yiran Wu***: Methodology. ***Dawei Sun***: Writing – review & editing, Investigation. ***Xin Zhang***: Writing – review & editing, Supervision, Resources, Project administration, Methodology, Funding acquisition, Conceptualization.

**DECLARATION OF COMPETING INTEREST**

The authors declare that they have no known competing financial interests or personal relationships that could have appeared to influence the work reported in this paper.

**ACKNOWLEDGEMENTS**

The authors are grateful for the financial support towards this research by the Chemical Engineering Department, College of Engineering, Tikrit University. Postgraduate Research Grant (PGRG) No.TU.G/2021/HIR/MOHE/ENG/39 (2895-7-3).

**عنوان البحث نوع الخط ايريل حجم 20 نقطة مع تجنب المختصرات**

**الخلاصة**

قد لا يعطي استعمال الملبدات التقليدية مثل كبريتات الالمنيوم المائية (الشب) الازالة المطلوبة للعكورة من مياه الفضلات الصناعية، هذا بالإضافة الى الحاجة الى وقت مكوث طويل نسبيا. تقنية التلبيد المغناطيسي احدى التقنيات الواعدة لغرض تقليل وقت المكوث والحصول على كفاءة إزالة اعلى للعكورة. في هذا العمل تم انجاز ثلاث مجموعات من التجارب لدراسة إمكانية رفع كفاءة إزالة العكورة وتقليل وقت المعالجة لمياة فضلات ماخوذه من مصفى الدورة حيث تم استعمال الشب مع كل من الملبدات المغناطيسية: أوكسيد الحديد والنيكل والكوبلت. كما تمت دراسة تاثير العوامل التشغيلية التالية: الدالة الحامضية، جرعة الشب، جرعة المادة المغناطيسية ونوع المادة المغناطيسية على كفاءة إزالة العكورة. بينت النتائج المختبرية ان هناك زيادة ملموسة في كفاءة إزالة العكورة ونقصان كبير في وقت المكوث نتيجة لاستعمال المواد المغناطيسية مع الشب. كما بينت النتائج المختبرية ان اعلى كفاءة إزالة للعكورة قد بلغت 99.88% عند دالة حامضية مقدارها 6.5 وذلك باستعمال جرع شب مقدارها 120 ملغم/لتر إضافة الى جرعة نيكل مقدارها 80 ملغم/لتر وذلك لنموذج عكورته الابتدائية 122 وحدة عكورة.

**الكلمات الدالة**: التلبد المغنطيسي ، مياه الصرف الصحي في معامل تكرير النفط ، النيكل ، الكوبالت ، أكسيد الحديد.

Add space before introduction, and don't use bullets list

اضف فراغا قبل المقدمة ولاتستخدم الترقيم التلقائي مطلقا وفي أي مكان من البحث

على الباحث رفع ملف واحد يحتوي على كافة التفاصيل (الاسم والخلاصة وأسماء الباحثين ومكان عملهم وايملاتهم و رقم اوريكد لجميع الباحثين والنقاط البارزة والخلاصة العربية والكلمات الدالة باللغتين)

Article Specialist (General): Put here Article Specialist (General)  
Article Specialist (in deep): Put here Article Specialist (in deep)

Select from here **Categories** **general** and **in-deep** specialist of your manuscript.

|  |  |
| --- | --- |
| * **Civil and Structural Engineering** * --->Structure * --->Construction Materials * --->Geotechnical engineering * --->Water Resources * --->Hydraulic Structures * --->Roads and Traffic * --->Projects Management * **Electrical and Electronic Engineering** * --->Power and Energy Systems * --->Communications and Signal Processing * --->Computer Engineering (hardware) * --->Control Systems * --->Mechatronics * --->Power Electronics * **Mechanical Engineering** * --->Applied Mechanics * --->Thermal powers * --->Manufacturing and minerals | * **Environmental Engineering** * --->Water pollution and treatment * --->Water quality management * --->Solid waste management * --->Soil pollution * --->Environmental disasters * --->Air pollution * --->Biodiesel production * --->Environmental monitoring * --->Climate change in the Environment * --->Sludge treatment * --->Noise pollution * --->Wastewater treatment * **Chemical Engineering** * --->Process Control * --->Transport Phenomena * --->Reactor Engineering and Catalyst * --->Petroleum Refinery Processes * --->Water and Wastewater Treatment * --->Mathematical Modelling and Simulation * --->Units Operation |

**Please Note:** Determining whether the research falls within the journal's scope is the responsibility of the authors. The authors should note that the initial evaluation of the research, based on which a member of the journal's editorial board refers the research to reviewers, does not mean that the research is entirely within the journal's scope. Reviewers, who are experts in the specific field of the research, may discover upon review that the research does not fall within the journal's scope. The journal is not responsible for the loss of time and effort resulting from the research not matching the journal's scope. Therefore, we advise researchers to read the instructions carefully and not to submit research that does not fall within the journal's scope.

ان تحديد هل البحث يقع ضمن تخصص المجلة يقع على عاتق الباحث ويجب على الباحث ان يلاحظ ان التقييم الاولي للبحث والذي بموجبه يقوم عضو هيئة التحرير في المجلة باحالة البحث للمقيمين لايعني ان البحث بالكامل ضمن تخصص المجلة اذ قد يكتشف المقيمين والذين هم ضمن التخصص الدقيق للبحث ان البحث بعد المراجعة لايقع ضمن تخصص المجلة. ان المجلة غير مسؤولة عن ضياع الوقت والجهد نتيجة عدم مطابقة البحث لتخصص المجلة وعليه ننصح الباحثين بقراءة التعليمات جيدا وعدم تقديم بحث لايقع ضمن تخصص المجلة.

Dear Editor,

I/We wish to submit an original research article entitled for consideration by Tikrit Journal of Engineering Sciences.

I/We confirm that this work is original and has not been published elsewhere, nor is it currently under consideration for publication elsewhere.

In this paper, I/we report on / show that**: Please explain in your own words the significance and novelty of the work, the problem that is being addressed, and why the manuscript belongs in this journal. Do not simply insert your abstract into your cover letter! Briefly describe the research you are reporting in your paper, why it is important, and why you think the readership of the journal would be interested in it.] nodality.**

We believe that this manuscript is appropriate for publication by your journal because it… **[specific reference to the journal’s Aims & Scope]**.

Please put here the thesis or dissertation name if the paper drawn from it: **Thesis or dissertation name**

**Please suggest at least three reviewers :**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Full name with title | Affiliation | e-mail | Phone number | Specialist |
| Reviewer 1 |  |  |  |  |  |
| Reviewer 2 |  |  |  |  |  |
| Reviewer 3 |  |  |  |  |  |

We have no conflicts of interest to disclose.   
Please address all correspondence concerning this manuscript to me at [email address].

Thank you for your consideration of this manuscript.

Sincerely,

[Corresponding Author name and Email]

**1.INTRODUCTION**

The manuscript should be font Georgia size 12 one column 1.5 line space with continues line number. The total number of pages must be up to 25 pages (include all figures, tables, references, ……. etc.)

Earlier studies show that an average of 468 gallons of water were required to refine one barrel of crude oil [1]. However, recent studies show that in USA one barrel of crude oil requires 42–79.8 gallons of water to be refined, with a median of 63 gallons of water[2]. Taking into account that 18.9 million barrels per day of crude oil is refined in USA at 2013 [3]*,*water reuse within an industrial plant is essential[4]. Wastewaters of the oil refineries contain a large quantity of solids, salts, crude oil, aromatic and cyclic hydrocarbons, surfactants, phenols, naphthalene acids, sulfides, heavy metals, and other chemical products. In primary purification of water and industrial wastewater treatment, a widely used process is coagulation–flocculation. This process is preferable in primary treatment due to its simplicity, high efficiency and cost-effectiveness [5]*.* However, this process exhibits several disadvantages, such as the need for high amounts of chemicals for neutralizing the charges of the suspended particles, the need for pH adjustment before and after treatment, the sensitivity to temperature change, in addition to the excessive sludge production [6]. Various improvements are introduced to the coagulation–flocculation process, such as using natural or synthetic polymers as a flocculant aids to strengthen flocs, employing another technology of separation with the coagulation–flocculation process, like magnetic flocculation. Its principle is adding particles of a higher magnetic susceptibility into a conventional coagulation – flocculation process to enhance the flocculation velocity and form flocs of high density to settle quickly [7]. It combines a traditional flocculation and a magnetic separation in one process exhibiting a quick, simple, energy – efficient, and cost effective advantages [8]**.**

Miura et al. [9] applied a ferromagnetic powder with aluminum sulfate or polyaluminum chloride in order to remove solids from the wastewater. They got a removal efficiency of 99%. It was noticed that the required time for separating flocculated suspended solids is only few seconds, while in conventional treatment, it takes about one hour. Slusarczuk and Brooks [10] added a magnetic ferric powder and polyethylene imine as a flocculant agent to treat the turbidity. It is found that ferrite powder exhibited synergism with the aqueous polyethylene imine solution. The results revealed that the sludge volume is about 80% less than the volume produced by using polyethyleneimine alone. The suspended solids removal efficiency is raised from 30% to 71 % when 1000 ppm of ferrite powder and 10 ppm of polyethyleneimine are added. Kang et.al. [11] used a magnetic ferrite powder of about 5 μm average particle size after dealing it with a solution of white alum (KAl(SO**4**)**2**), polyaluminum chloride or ferric chloride. Ferrite powder was added at stirring speed of (200 - 300 rpm) for (1.0 - 2.0 minutes). It was found that the flocculated particles settled rapidly at a rate of 5 cm/minute, whereas in conventional methods that use alum or polyaluminum chloride, a period of 2.0-4.0 hours is required for efficient settling.Magnetic seeding aggregation (MSA) of silica nanoparticles was studied by Ref. [12]*.* Influences of pH, salts addition, and type of magnetite seeding particles on the turbidity removal efficiency were examined. The turbidity of CMP treated wastewater is reduced from 110.0 NTU to 7.0 NTU at pH of 6. The results showed that the residual turbidity decreases with the increase of magnetic field intensity. When the magnetic field intensity is higher than 0.08 Tesla, the residual turbidity is about 1.0 NTU. High turbidity reduction during the storm period by magnetic aggregation and separation was obtained by Ref. [13]*.* High turbidity raw water was prepared by mixing a sludge sample that are taken from Shiemen reservoir's tail water pond with deionized water. It was found that at magnetic field strength of 0.1 Tesla, the magnetic aggregation effects were not significant but at magnetic field strength of 0.15 Tesla, significant effects on the magnetic aggregation were observed. When the magnetic field strength raised to 0.2 Tesla, the effect on magnetic aggregation was stable. The results also showed that with increasing the magnetite dosage from 2880 mg/L to 3360 mg/L, the final turbidity is reduced from 130 NTU to 20 NTU, while raising the magnetite dosage from 3360 mg/L to 4800 mg/L, the final turbidity is decreased from 20 NTU to 18 NTU. It was found that the turbidity removal efficiency at pH of 8.0 was superior than that at pH of 6. Akbar et al. [14]proved thatturbidity removal is affected by pH, coagulant dosage, as well as initial turbidity. They found that the highest turbidity removal fall within 82-99.4% for initial turbidity of 10-1000NTU at pH of 5-7 and coagulant dose of 10-20mg/L. Ching and Zhen [15] conducted a study on magnetic seeding aggregation of high turbid source water as a pretreatment process using magnetite nanoparticles. The effect of pH on turbidity removal efficiency was studied over pH range of 5.0-9.0 and magnetic field strength of 0.0 Tesla to 0.1 Tesla. It was found that the final turbidity is decreased with the increase of the magnetite dosages. They got a turbidity of 774, 240, 56,19 and 10 NTU when using 1.0, 3.0, 5.0, 7.0 and 9.0 g/L magnetic dose. Their results showed that at pH values of 5.0, 6.0, 7.0, and 8.0 give the residual turbidities of 80, 234, 36 and 128 NTU, respectively. Mann [16] treated North Saskatchewan River water with different concentration of combination magnetite nanoparticles, aluminum sulfate and polyacrylamide. Turbidity test reported that, 300 mg/L magnetite nanoparticles has the highest removal efficiency of 98%. It was found that the required time for removing the turbidity using magnetite is 10 minutes, while by using aluminum sulfate and polyacrylamide combination, it is 30 minutes. Basma and Hussein [17]found that turbidity removal depends mainly on the coagulant dose, pH, and settling time. They found that the turbidity could be reduced from 92 to 2.1NTU at pH of 6, coagulant dose of 80 mg/L, and 120 minutes settling time.The feasibility of turbidity removal using a high gradient superconducting magnetic separation was studied by Ref. [18]*.* The process variables are, polyaluminum chloride (PAC) and magnetic seeds dosages. The initial turbidity of wastewater is 110 NTU, and the applied magnetic field intensity is 5.0 Tesla. A study regarding the use of a flocculated magnetic separation technology for treating Iraqi oilfield co-produced water for injection purpose was accomplished by Al-Rubaie et al. [19]*.* Results revealed that effluent water with low suspended solids and oil content can be obtained by applying a flocculation magnetic separation. It was also found that the required time for settling, several times less than that of the conventional methods. Treating of the emulsified oil wastewaters using a modified Fe**3**O**4** magnetic nanoparticles MNPs, was made by Ref. [20]*.* A chitosan grafted magnetic nanoparticles Fe**3**O**4** @APFS MNPs was used. They found a good demulsification effect via electrostatic attraction. It was also found that the demulsification performance could be further more enhanced upon Chitosan grafting especially under alkaline condition.

In the present study, an investigation on applying magnetic flocculation to treat wastewater of Al-Doura oil refinery using iron oxide, Nickel, and Cobalt magnetic powders with alum is made. The main objectives of this study are: Increasing the removal efficiency of the suspended solids and reducing settling time and consequently treating large quantities of polluted water without a need for enlarging the treatment basin.

**2.EXPERIMENTAL PROGRAM**

Add space before and after

**2.1.*Apparatus and Procedures***

The Jar test apparatus was used in this study, is pharma test PT-DT7, it was taken from Samarra’a Company for drug and medical implementations (SDI).

***2.2.Experimental Procedure***

Add space before and after

The experimental procedures are listed below:

1. Beakers of 1000 ml are filled with 500 ml of wastewater after measuring its initial turbidity and adjusting the pH to the required value using 1.0 N HCl or 1.0 N NaOH.

2. The required magnetic powder dose was mixed with the wastewater at mixing speed of 250 rpm for 1.0 minute.

3. The required alum dose was added with rapid mixing of 200 rpm for 1.0 minutes, followed by a slow mixing of 30 rpm for 10 minutes. Then, the mixers are turned off and the magnets are attached to the beaker bottom from the outside for 5.0 minutes.

4. Pipette water sample from the supernatant to measure the final turbidity.

Note: When alum is used alone, the settling time is 30 minutes while 5 minutes is a settling time for all magnetic powder.

***3.3.Experimental Sets***

Add space before and after

Three sets of experiments were examined. In the first set, all experiments were conducted using a wastewater sample of initial turbidity 47.97 NTU, initial pH of 7.49, and temperature of 19.7 ºC. Five levels of alum dose (60, 80, 100, 120, and 140 mg/L), three levels of pH (5.5, 6.5, and 7.5), and three levels of magnetic material dose (160, 200, 240mg/L) for each one of iron oxide nanoparticles (Fe3O4), nickel (Ni), and cobalt (Co) are performed. The second set was performed in order to test the possibility of reducing the dose of magnetic materials. In this set, wastewater samples which had an initial turbidity of 49 NTU, initial pH=7.60, and temperature equal to 23ºC is used. In the third set the effect of initial turbidity (49, 61, 90, and 122 NTU) on the turbidity removal efficiency were tested after determining the best alum dose at pH of 7.

Wastewater samples had been taken from the industrial wastewater unit of Midland Refineries Company (Al-Doura Oil Refinery), precisely before the inlet of the coagulation-flocculation unit. Table 1 includes the operating variables for these sets.

Add space before table tittle

using align lift

**Table 1** Operating parameters values of the present work. (font size 10 point with Capitalize Each word)

|  |  |  |  |
| --- | --- | --- | --- |
| **Variable** | **Unit** | **Min. value** | **Max. value** |
| Consumptive use (Cu) | mm/day | 0.76 | 9.50 |
| Water Holding Capacity (W.H.C) | mm/cm | 0.3 | 1.5 |
| Root Zone Depth (R.Z.D) | cm | 60 | 100 |
| Depletion Percentage (Dp) | % | 70 | 70 |
| Application Efficiency (Ea) | % | 80 | 92 |
| Roughness Coefficient (n) |  | 0.04 | 0.25 |
| Available Discharge (Qa) | lit/sec | 2000 | 10000 |
| Conveyance Efficiency (Ec1) | % | 95 | 95 |
| Conveyance Efficiency (Ec2) | % | 90 | 90 |

add space after table

Before new paragraph tittle add space

**3.RESULTS AND DESCUSSION**

***3.1.Results of First Set***


These results are listed in Tables 2-4 and samples of these results are presented graphically.

**Table 2** Experimental Results of the First set for Iron Oxide.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Statistical evaluation types** | **Calibration stage** | | | **Validation stage** | | |
| **MLP** | **RBF** |  | **MLP** | **RBF** |  |
| R2 | 0.99 | 0.86 |  | 0.96 | 0.89 |  |
| MAE | 18.63 | 68.62 |  | 16.79 | 42.58 |  |
| RE | 0.07 | 0.22 |  | 0.08 | 0.36 |  |
| NSE | 0.99 | 0.66 |  | 0.94 | 0.66 |  |

If (figure) in start sentence, otherwise, using Fig. of Figs.

Figures. 1 and 2 represent the effect of pH on turbidity removal efficiency using alum alone and alum with 160 mg/L of iron oxide respectively. These Figures show that low turbidity removal efficiencies are obtained at pH=5.5, while high turbidity removal efficiencies are gained at pH=6.5 and pH=7.5. These pH values which give the highest turbidity removal are within the range of operating region for alum precipitation which is from 5.0 to 7.0 with minimum solubility occurring at pH equal to 6.0 [4]. Similar trend was obtained by [14, 17, 21]. Lo et al (2007) reported that the surface of the magnetite particles is positively charged at pH=6.0. Hence, at Fe3O4 doses equal to 160 mg/L and 200 mg/L the net charge of the wastewater will be positive so, a steric repulsion in the solution is occur, so high residual turbidity will remain, but at Fe3O4 dose =240 mg/L the weighting effect predominates and overcomes the electrostatic repulsion forces. For aluminum-based coagulants, the best coagulation performance is generally observed at pH values that are as close as possible to the pH of minimum solubility of the coagulant [22]*.*




the equation no. inside equation

and using align right

equation without bold

Finally, Eq. (1) may be rearranged as follows:

Add space before and after equation



The optimum pH value depends on the treated water properties, coagulant type, and coagulant concentration[23]**.** Similar trend was obtained for all magnetic powder, as it is clear from Tables 2 - 4 which indicate that the higher removal efficiency for all magnetic powders was obtained at pH 6.5 and 7.5. It is also clear that 200 mg/L of Nickel with 60 mg/L alum at pH of 7.5 gave the highest removal of 98.45% while the highest removal for 240 mg/L iron oxide (97.89%) was obtained at pH of 6.5 and 80mg/L alum and the highest removal for 240 mg/L of Cobalt was (97.22%) obtained at pH of 6.5 and 100 mg/L alum. Effect of pH on turbidity removal efficiency at different alum dose can be shown in Fig.2.

The avarage free heat transfer coefficient the following expression is obtained [18]:

Fig. 3 describes the influence of alum dose on turbidity removal efficiency at different pH values by applying alum only. It is clear that the removal efficiency increases with the increase of alum dose up to a certain limit then it drops. These results are in well agreement with that of [17, 24] who reported that colloidal particles are negatively charged and upon addition of aluminum sulfate, Al+3 ions are attracted to these particles. At the point of a complete charges neutralization, the colloids begin to agglomerate due to a collisions between particles. If excess coagulant is added to the wastewater, the results are a reverse of the net charge on the colloidal particles (from negative to positive).

add space before figure

**Fig. 5** Determination Coefficients () for the Width of the Basin using MLP and RBF Models. (font size 10 point with Capitalize Each word)

add space after tittle of figure

Using insert eqution for subscript, below or above in the main text

Particle re-stabilization by a reversal charge allowed greater amounts of smaller particles to remain in solution, thus increasing the total solids. Excess alum dose may exceeds the saturation limit or produce excess aluminum hydroxide and thus will be a source of turbidity so the removal efficiency will be decreased [4]*.* The highest removal (96.12%) is obtained at 100 mg/L alum dose at pH of 6.5. The best removal (77.58%) at pH of 5.5 is obtained for alum dose of 80 mg/L, while at pH of 7.5 and alum dose of 120 mg/L the highest removal is 95.08%. These results show that the relationship between pH and alum dose is proportional. This may attribute to the alkalinity of the treated water. Metal coagulants are acidic, therefore, coagulant addition consumes alkalinity. In the case of   
pH =5.5 low dose of alum is required to get good results, since a high dose of alum will consume all the available alkalinity, lowering the pH to too low values for efficient treatment. When pH=7.5, high dose of alum is required to depress the pH (reduce the alkalinity) to a favorable values for coagulation. At pH=6.5, an optimum alum dose and a best removal efficiency are obtained. This value is within the operating region range for alum precipitation which is from 5.0-7.0 with minimum solubility occurring at pH equal to 6.0 [4]*.*

Fig. 4 describes the influence of alum dose on turbidity removal efficiency at different pH values with the presence of 240 mg/L of Nickel. Inspection of this Figure and Tables 2–4 indicate that the general trend is nearly constant and the effect of alum dose with the presence of magnetic powder is little. Turbidity removal efficiency is increased slightly with the increase of alum dose at pH of 5.5 while it decreased slightly with the increase of alum dose at pH of 6.5 and 7.5. Moreover, the highest turbidity removal for alum alone or alum with any of the three magnetic materials is obtained at pH of 6.5 and 7.5 which are close to each other and the lowest removal was obtained at pH of 5.5. As mentioned previously, at low pH higher alum dose is required to get good results, since a high dose of alum will consume all the available alkalinity, lowering the pH to too low values for efficient treatment. When pH=7.5, high dose of alum is required to depress the pH (reduce the alkalinity) to a favorable value for coagulation [4]*.*However, at pH of 6.5 and 7.5, there is a slight decrease of removal efficiency with the increase of alum dose***.*** This is for two reasons; the first is excess alum dose may exceed the saturation limit or produce excess aluminum hydroxide and thus will be a source of turbidity so the removal efficiency will be decreased [4] and the second is the fact that high magnetic powder dosage does not mean better efficiency, it becomes a source of turbidity that is extremely difficult to be removed without externally applied magnetic field. While at low dosage of magnetic powder, the effectiveness of magnetic aggregation will be poor [13]*.* This Figure show that the main effect is for pH and magnetic powder.

**Fig. 6** Determination Coefficients () for Basin Discharge using MLP and RBF Models.

Three levels of magnetic powder dose were used namely; 160, 200, and 240 mg/L. Figs. 5–7 represent samples of the results for iron oxide, Nickel, and Cobalt that gives the highest removal efficiency respectively. A careful inspection of these figures and Tables 2–4 clarify that turbidity removal is increased with the increase of the magnetic powder dose up to a certain limit then it drops slightly. These results are in agreement with that of [25]. The lowest removal takes place at pH of 5.5 and the highest removal takes place at pH 6.5 or 7.5. Moreover, the removal at pH 6.5 and 7.5 are close together for all magnetic powder except Cobalt. Also, it could be found that the magnetic powder value that gives the highest removal depends on both pH and alum dose. The optimum performance for turbidity removal depends on pH, treated water properties, coagulant type, and coagulant concentration [23]. Appropriate magnetic powder dosage is crucial, high dosage does not mean better efficiency, it becomes a source of turbidity that is extremely difficult to be removed without externally applied magnetic field, in addition to high amounts of sludge formation. While at low dosage of magnetic powder, the effectiveness of magnetic aggregation will be poor [13]*.* The highest turbidity removal of 98.45% is obtained when using 200mg/L of Nickel with 60 mg/L alum at pH of 7.5.

***3.2.Second Set of Results***

Since the best pH is 6.5 and 7.5 according to the results of the first set, thus it was decided to take the average value (7) to determine the best alum dose at this average value of pH. It was found that 120 mg/L of alum gives the highest removal efficiency (Fig. 8). This alum dose is used to find the effect of pH on removal efficiency and it is found that the pH range 6.5-7.5 gives the highest removal. However at pH of 6.5, the highest removal is obtained (97.87%)(Fig. 9).

This result is in agreement with that of [26]. Then, in a trial to test the possibility of reducing the magnetic powder dose, it is decided to use a range of 40 to 120 mg/L for each of the three magnetic powders. The results were presented on Fig. 10. It is clear that at low doses of magnetic powders the removal efficiencies are low and it increases with the magnetic powder dose increase. At low dosage of magnetic powder, the effectiveness of magnetic aggregation will be poor [13]*.* It could be seen that the best Fe3O4 magnetic powder dose is 120 mg/L, while for nickel and cobalt they are 80 mg/L and 100 mg/L respectively. The optimum performance depends on pH, treated water properties, coagulant type, and coagulant concentration [23]. It could be concluded that nickel magnetic powder exhibits an excellent performance, where its optimum dose is low in comparison with iron oxide and cobalt and it gives a removal efficiency reaches to 98.57%. Effect of pH on turbidity removal, Alum dose= 120 mg/L can be shown in Fig.9.

***3.3.Results of the Third Set***

After finding the best conditions of alum dose, pH, and magnetic doses, an evaluation for using different initial turbidities with the best findings are illustrated in Fig. 11.

Using insert eqution for subscript, below or above in the main text without italic

It is clear that for alum alone, and alum with , the turbidity removal start to fall down at an initial turbidity of 61 and 90 NTU respectively, while Cobalt and Nickel still show good results at higher turbidities. This was found is in full agreement with that of [14] who stated that turbidity removal efficiency is decreased to a certain extent by increasing initial turbidity and application of higher coagulant dosage may improve turbidity removal from relatively high turbidity waters since high turbidity in addition to the dispersed Fe3O4 will need a lot of alum doses to neutralize their charges and overcome the mutual repulsion forces between suspended solids. They also found that there is an optimum magnetic dose for a specific initial turbidity range. However, when the raw water turbidity is altered, this optimal dosage will require an experimentally adjustment. They found that the optimum magnetic dose shows a linear relationship with the initial turbidity. They stated that the coagulation process and turbidity removal was considerably affected by pH, coagulant dosage, as well as initial turbidity.[Bahman (2014)[25]](https://www.sciencedirect.com/science/article/pii/S2212371714000171" \l "!)[reported that](https://www.sciencedirect.com/science/article/pii/S2212371714000171" \l "!)the increase in the turbidity removal with the increase of the initial turbidity might be attributed to other mechanisms such as sweeping flocculation rather than the neutralization of the surface charge of colloids.

For all experiment when using alum with magnetic powder, samples for the determination of removal efficiency are taken after 5 minutes while for alum only, samples are taken after 30 minutes of settlement. The removal efficiency when using alum (100 mg/L) and Fe3O4 (160 mg/L) at pH of 7.5 is 96.66% after 5 minutes settling while with employing alum only the turbidity removal efficiencies are 67.91% and 93.67% at settling periods of 5.0 minute and 30 minutes respectively. This finding can give an increase of the treated volumes by 6 folds which is an essential matter for the field units.

Finally, from the present work results, it could be concluded that, there is no specific value for the independent variables that gives the best results. Therefore, these values should be determined for each case depending on the experimental laboratory results. It is also revealed that the nickel magnetic powder with alum give the best results by a comparison with and cobalt magnetic powders.

**4.CONCLUSIONS**

The main conclusions of the present study could be summarized as follows:

* An enhancing in the turbidity removal efficiency is achieved by utilizing magnetic flocculation technique.
* The required period for settling is very short (five minutes) in comparison with conventional method.
* There is a potential for applying the same operating conditions for various initial turbidities, but in reasonable limits.
* It can be concluded that nickel magnetic powder has a superior performance in comparison with iron oxide and cobalt magnetic powders.
* The maximum turbidity removal efficiency is 99.88% when applying magnetic flocculation technology, while with applying conventional flocculation the maximum turbidity removal efficiency is 92.89 % at the same conditions.

The manuscript must include Achnowledgement

**يجب ان يحتوي البحث على فقرة العرفان بالجميل** ، البحوث التي لاتحتوي على هذه الفقرة سوف تهمل

رقم التمويل المالي المذكور هنا يقصد به الامر الجامعي بقبول الطالب في الدراسات العليا اذا كان البحث بحث طالب دراسات، اما اذا كان الباحث تدريسي فيقصد به الامر او القرار الخاص بإقرار البحث في الخطة البحثية

او التمويل المالي الخاص من أي جهة ممولة.

البحوث التي لاتحتوي على هذه الفقرة تهمل الا اذا كان البحث ممولا بالكامل من قبل الباحث وقد تحمل الباحث أجور الدراسة والمحاضرات والاشراف وشراء الأجهزة على حسابه الخاص واجور تشغيل الأجهزة والكهرباء والصيانة والحراسة وشراء المواد ودفع للجامعة أجور الموافقة على وضع اسمها على البحث. في هذه الحالة يكتب في هذه الفقرة البحث ممول بالكامل من قبل الباحث، مع ارفاق كتب من الجامعة يبين فيه ان البحث ممول بالكامل من قبل الباحث، بخلافه يعتبر البحث ممولا من الجامعة بمجرد صدور الامر الجامعي بقبول الطالب في الدراسات العليا او صدور ادراج البحث ضمن الخطة البحثية للقسم

**NOMENCLATURE**

*A* Area,

*Cp* Specific heat capacity, J/(kg )

*D* Cylinder diameter, m

*g* Gravitational constant, m/

*h* Heat transfer coefficient, W/()

*I* Current, A

*k* Thermal conductivity, W/(m )

*L* Fin length, m

*N* Fins number

*Nu* Nusselt number

*Q* Input heat, W

R Fin radius, m

*Ra* Rayleigh number

Thermal resistance, /W

*t* Fin thickness, m

*T* Temperature,

***Greek symbols***

Thermal diffusivity, /s

Expansion coefficient, 1/K

Dynamic viscosity, kg/(m s)

Kinematic viscosity, /s

Density, kg/

Emissivity

Input voltage, V

***Subscripts***

*b* base

*in* input

ambient

TJES has ref Style, please read Author Guidelines carfully before complete Refs list

المجلة لها ستايل مصادر خاص بها لايشبه أي مجلة أخرى ، كما ان هناك ملف ستايل خاص ببرنامج ايند نوت وبرنامج مندلي موجود في موقع المجلة

[Guide for Authors – Copy – Tikrit Journal of Engineering Sciences](https://tj-es.com/guide-for-authors-copy/)

يجب قراءة تعليمات النشر جيدا قبل اعداد قائمة المصادر ، كذلك فان الأمثلة التالية تعطي امثلة لاهم المصادر

**REFERENCES**

1. Mousa KM, Hadi HJ. Coagulation/flocculation process for produced water treatment. *International Journal of current Engineering and Technology* 2016; **6**(2): 550-555.
2. Tahseen TA, Ishak  M, Rahman  MM. **Performance predictions of laminar heat transfer and pressure drop in an in-line flat tube bundle using an adaptive neuro-fuzzy inference system (ANFIS) model**. *International Communications in Heat and Mass Transfer* 2014; **50**(1): 85–97.
3. Strunk JW, White EB. The elements of style. 4th ed., New York: Longman; 2000.
4. Kaviany M. Heat transfer in porous media. In: Rohsenow, WM, Hartnett, JP, Cho, YI, (Eds.), Handbook of Heat Transfer. New York, USA: McGraw-Hill; 1998.
5. Tahseen TA, Gaeid KS, Ajel AR, Mahdi MS. Performance prediction for forced convection in an equilateral triangular channel based on intelligent control. *1st International Conference for Engineering Researches* 2017 Mar 1-2; Baghdad, Iraq. Middle Technical University: p. 10-17.
6. Mohammed MM. A hybrid CFD-ANN approach to analysis heat transfer laminar flow across flat-tube banks. M.Sc. or Ph.D. Thesis. Tikrit University; Tikrit, Iraq: 2016.
7. Davids J, Smith D. Analysis of constant-velocity joints under high torque. HMSO: London; 1996: pp. 1-8.
8. Tahseen TA. How to write and published the impact factor journals. Tikrit University; Tikrit, Iraq. 2018: Available from: <http://en.tu.edu.iq/>
9. Trainham JA, Hoertz PG, Bonino CA, Newman JS. Particulate heat transfer fluid and related system and method. The USA, patent No. US 9651313 B2; 2017: 1-47.